


Step-by-Step Instructions

Portable Metal Frame Sneeze guard

**Step 1:** Peel off the blue protective tape on both sides being careful not to scratch.



**Step 2:** Set both stands so that they face each other, as pictured.

**Step 3:**

Unscrew the 4

white screws on the top of the stands



**Step 4:** Gently place shield on the stands, and continue to insert the white screws back to their original positions.

**Step 5:** Loosen left and right wingnuts until shield is in desired position, then tighten



**Step 6:** Loosen left and right tensioner to adjust height to desired position, then tighten.

That’s It!

